|  |
| --- |
| **Configure Samba** |
| etc/samba/smb.conf. Add the below lines to the profile section right above the printers |
| [Snickerdoodle]  path = /snickerdoodle  guest ok = yes  browsable = yes  create mask = 0775  directory mask = 0775  read only = no  force user = root  force group = root |
| cd /etc/init.d |
| service smbd start |

Then create snickerdoodle directory with mkdir /snickerdoodle